
***********************************************************************
 ZEBRA Monitor
 Installation informations

23 May 2011
***********************************************************************



***********************************************************************
 WARNING: read carefully the following informations
 before proceeding with ZEBRA Monitor installation.
***********************************************************************

* To install ZEBRA Monitor run the setup program ZM_Setup_vXXX.exe.
  This program will install before also all necessary drivers for PCAN
  and Vector hardware. In order to repeat manually the drivers
  installation, please follow the next step, otherwise skip it.

* Be sure to have installed CAN hardware interfaces drivers before this
  installation, otherwise ZEBRA Monitor could not work properly!
  In order to do this follow the instruction in:
  - PEAK-SYSTEM: CD-ROM\DiagnosticKit_CD_v2.7xxx\CAN\Peak
  - VECTOR: CD-ROM\DiagnosticKit_CD_v2.7xxx\CAN\Vector
  IMPORTANT NOTE: read carefully the installation notes of each included
  driver. Some interfaces are restricted to be used only in particular
  Operating Systems! (CancardX can't work with MS Vista)
  Be aware that the use of last version of drive is reccomended.

* To install ZEBRA Monitor upgrades ('Upgrades' folder), if included in
  the CD-ROM, simply copy the upgraded executable (usually named as
  ZEBRAmonitor_Vxxx_Ly.exe) into the same folder of the basic installation.
  In the folder upgrades is present a demo version useable only to work
  off line without connected BMI.
  
  In the file name there is the ZMversion; the level: 0, 1semplified, the
  type of use Local or remote; only for remote mode the option full or light.

* When ZEBRA Monitor is executed the first time, it will ask to select the
  target CAN hardware interface. The hardware can be changed also during
  the execution.

* Please, never remove the files included into the following folder:
  <Program Files>\Common Files\ZEBRA Monitor.

* If WinFlash application is included in this installation package, please
  follow the installation note in:
  D-ROM\DiagnosticKit_CD_v2.7xxx\WinFlash

* When ZEBRA Monitor is used in remote mode, it is necessary an internet
  connection with a static IP and an opened port (i.e. 23480).
  Zebra monitor in remote mode can be in Full or Light version.
  The light version doesn't allow some function like: BMI reset, 
  set manual switch off error, change BMI address-charger type, BMI's sn,
  update constant, download receipe, start from ZM the electric
  ISO test-fan test-send system enable.
 
  To perform a connection to a remote vehicle, follow the steps below:
  1) Specify the vehicle identification number (usually the telephone number
     of the SIM inside the localizator using the international prefix 00xx...)
     in the system configuration dialog box of ZM.
  2) Send the following SMS to the SIM inside the localizator:
     connect <ZM_STATIC_IP> <PORT>
     where <ZM_STATIC_IP> is a valid static IP used to reach the PC where
     ZM is running, and <PORT> is the number of the service port used to
     communicate with ZM, generally the 23480.


***********************************************************************
FIAMM SONICK sa
 Via Laveggio 15 - CH 6855 STABIO - SWITZERLAND


 General contacts:
 Phone:  +41 (0)91 6415311
 Fax:    +41 (0)91 6415395
 e-mail: info@fzsonick.com
