***********************************************************************
 Peak CAN-USB hardware interface
 Installation Notes

 10/12/10
 Operating systems: Windows 2000 SP4, XP, Vista, 7

 Copyright "PEAK-System Technik GmbH" - All rights reserved.
***********************************************************************

Follow these steps in order to install properly Peak CAN-USB interface:
(in this case will be updated the drivers for PEAK at version 3.4.0.9248)

1. In order to install properly the Peak CAN driver, run the setup program:
   CD-ROM\DiagnosticKit_CD_v2.7xxx\CAN\Peak\PCANdrv\InstallPCANdrv.exe

2. From CD-ROM\DiagnosticKit_CD_v2.7xxx\CAN\Peak 
   execute "PcanDrv_FzSonick.exe" (without plugging PEAK into USB port).
   
   WARNING:
   This software must be installed and used ONLY for this application: no
   farther use or distribution is permitted.
   FZ Sonick will not be responsible in case of an use not licensed.

3. Now the driver will be installed.

4. Plug the interface into an available USB port of the computer and wait
   that the system will finish the installation.

5. Verify that in Control Panel the "CAN Hardware" applet has
   "Active Device" = "USB", otherwise select "USB".

6. Now the interface will be correctly installed. 


***********************************************************************
 FZ Sonick sa
 Via Laveggio 15 - CH 6855 STABIO - SWITZERLAND

 General contacts:
 Phone:  +41 (0)91 6415311
 Fax:    +41 (0)91 6415333
 e-mail: info@fzsonick.com

*************************************************************************